#compdef tcpdump

typeset -A opt_args

_interfaces () {
	_wanted interfaces expl 'network interface' \
		_net_interfaces
	_values "Pseudo-device that captures on all interfaces" "any"
}

_esp_secrets () {
	_values -S : 'ESP algorithm' \
		'des-cbc:secret' \
		'3des-cbc:secret' \
		'blowfish-cbc:secret' \
		'rc3-cbc:secret' \
		'cast128-cbc:secret' \
		none
}

_packet_types () {
	_values 'Packets type' \
		'aodv[Ad-hoc On-demand Distance Vector protocol]' \
		'cnfp[Cisco NetFlow protocol]' \
		'rpc[Remote Procedure Call]' \
		'rtp[Real-Time  Applications  protocol]' \
		'rtcp[Real-Time Applications control protocol]' \
		'snmp[Simple Network Management Protocol]' \
		'tftp[Trivial File Transfer Protocol]' \
		'vat[Visual Audio Tool]' \
		'wb[distributed White Board]'
}

_data_link_types () {
	if (( $+opt_args[-i] )); then
		vals=( ${${${(s:  :)"$(_call_program data-link-types tcpdump -L -i $opt_args[-i] 2>&1)"}[2,-1]}/ /:} )
		_describe -t data-link-types "data link types ($opt_args[-i])" vals && ret=0
	else
		_values "Data link types (general)" \
			"EN10MB" \
			"LINUX_SLL"
	fi
}

_bpf_filter () {
}

_arguments \
  '()-A[print each packet in ASCII]' \
  -c'[exit after receiving specified number of packets]:number of packets' \
  -C'[specify output file size in MB (10e6 bytes)]:output file size' \
  '(-ddd)-d[dump the compiled packet-matching code in a human readable form]' \
  '(-ddd)-dd[dump packet-matching code as a C program fragment]' \
  '(-d -dd)-ddd[dump packet-matching code as decimal numbers (preceded with a count)]' \
  '(-A -c -C -d -dd -ddd -e -E -f -F -i -l -L -m -M -n -N -O -p -q -R -r -S -s -T -t -tt -ttt -tttt -u -U -v -vv -vvv -w -W -x -xx -X -XX -y -Z *)'-D'[print the list of the network interfaces available on the system]' \
  -e'[print the link-level header on each dump line]' \
  -E"[decrypting IPsec ESP packets]:spi@ipaddr::algo\:secret:_esp_secrets" \
  -f"[print 'foreign' IPv4 addresses numerically]" \
  -F'[input file for the filter expression]:filter expression file:_files' \
  -i'[interface]:interface:_interfaces' \
  -l'[make stdout line buffered]' \
  '(-A -c -C -d -dd -ddd -e -E -f -F -l -D -m -M -n -N -O -p -q -R -r -S -s -T -t -tt -ttt -tttt -u -U -v -vv -vvv -w -W -x -xx -X -XX -y -Z *)'-L'[list the known data link types for the interface]' \
  '*-m[load SMI MIB module definitions]:SMI MIB module definitions:_files' \
  -M'[shared secret for validating the digests in TCP segments with the TCP-MD5 option]:secret' \
  -n"[don't convert addresses to names]" \
  -N"[don't print domain name qualification of host names]" \
  -O"[don't run the packet-matching code optimizer]" \
  -p"[don't put the interface into promiscuous mode]" \
  -q'[quick (quiet?) output]' \
  -R'[assume ESP/AH packets to be based on old specification (RFC1825 to RFC1829)]' \
  -r'[read packets from file]:input file:_files' \
  -S'[print absolute TCP sequence numbers]' \
  -s'[specify number of bytes of data to snarf from each packet]:number of bytes to snap' \
  -T'[interpret captured packets as specified type]:packet type:_packet_types' \
  "(-tttt)-t[don't print a timestamp on each dump line]" \
  '(-ttt -tttt)-tt[print an unformatted timestamp on each dump line]' \
  '(-tt -tttt)-ttt[print a delta (in micro-seconds) between current and previous line on each dump line]' \
  '(-t -tt -ttt)-tttt[print a timestamp in default format proceeded by date on each dump line]' \
  -u'[print undecoded NFS handles]' \
  -U'[make output packet-buffered when saving to file (-w)]' \
  '(-vvv)-v[slightly more verbose output]' \
  '(-vvv)-vv[more verbose output]' \
  '(-v -vv)-vvv[most verbose output]' \
  -w'[write the raw packets to file]:output file:_files' \
  -W'[limit the number of created files (-C)]:number of files' \
  -x'[print each packet (minus its link level header) in hex]' \
  '(-x)-xx[print each packet, including its link level header, in hex]' \
  -X'[print each packet (minus its link level header) in hex and ASCII]' \
  '(-X)-XX[print each packet, including its link level header, in hex and ASCII]' \
  -y'[set the data link type to use while capturing packets]:data link type:_data_link_types' \
  -Z'[drops privileges (if root) and changes user ID (along with primary group)]:user:_users' \
  '*:BPF filter:_bpf_filter'
